***ABSTRACT***

**ABSTRACT**

Vision is the most beautiful and vital gift from nature to all his creatures especially for human beings. But unfortunately there are some people who lack this beauty and are unable to capture the beauty of this world from their own eyes. Third eye for blind is a development which involves various areas such as, IoT, hardware and software integration and automation that enables visually impaired persons to see and explore the world confidently and independently by recognizing the nearby objects by using ultrasonic waves and inform the person with a beep ring or vibration.

As per WHO(world health organisation) 2.2 billion people suffer from vision impairment. They are facing troubles in their lifestyle. This device can act as an innovation for the visually impaired people. Due to their of vision, they find it difficult to navigate in public. They always require aid of different person for navigating in dense population. They also sometimes get into danger due to their vision impairment.

***INTRODUCTION***

**CHAPTER 1**

**INTRODUCTION**

As per the definition of blindness, we mean the person without sense of sight. A blind person has no ability to see anything. While struggling for the different levels of comforts of the general population, we have reached to a point where we have started to completely ignore the people who are living a miserable life due to lack of vision. They face enormous challenges in their daily lives and hence end up living a dependent life. They experience a completely different life from the normal people and experience detached and uninterested conduct towards them for being physically disabled. They need other individuals for their movement from one place to another.

Sight is the basic sense of life and therefore a person’s movement from place to place in this condition is a major challenge for the visually impaired . The target of this task , This project for the blind or visually impaired person will provide a gadget that is helpful to them as well as the persons who depend on any individual due to lack of sight. Third eye for blind task can be an innovation for the sightless individuals, it will help them to move from here and there and among different places with confidence by knowing the nearest obstructions while wearing the band which leaves the ultrasonic waves which inform the person with beep-sound or vibration. It can let the person who is not able to move and distinguish even snags due to lack of vision. They just have to put on the gadget as a spectacle which is part of their accessories. As per WHO(world health organisation) 2.2 billion people suffer from vision impairment. They experience a lot of troubles in the daily lives. This device can be an innovation for the physically disabled or blind individuals.

***SYSTEM STUDY***

**CHAPTER 2**

**SYSTEM STUDY**

**2.1 EXISTING SYSTEM:**

* on Applied Information Technology 7-9 October, 2015
* 213
* SMS
* Mess

There are three major existing system which are widely used by blind. They are:

* White Cane
* Vision (a torch for blind).
* Vibration gloves.

**2.1.1 WHITE CANE**

White Cane is a long stick used by blind to scan their environment. It is also difficult to handle in busy traffic. White Cane also causes huge inconvenience to general public.

**DISADVANTAGE**

* May crack or break easily.
* The stick may get stuck at the foot path cracks.
* Difficult to handle at crowded place.
* High chances for getting missed.

**2.1.2 VISION (A TORCH FOR BLIND)**

Vision is a smart device which consists of ultrasonic sensor which resides inside a box. When an object is detected, buzzer sound is produced. The blind has to carry the box manually. The whole system is controlled by a micro controller such as Arduino, Arduino nano, ESP 32., etc.

**DISADVANTAGE**

* Difficult to carry.
* High chances of getting dropped.
* Inconvenient to use.

**2.1.3 VIBRATION GLOVES**

This system consists of a glove attached with ultrasonic sensor. When an object is detected vibrator motor produces vibration that notifies the blind. The entire system is controlled by a micro controller such as Arduino, Arduino nano, ESP 32.,etc.

**DISADVANTAGE**

* Difficult to handle
* Difficult to perform other works wearing the gloves
* May cause strain in the client hand.

**2.2 PROPOSED SYSTEM**

We are going to build a system that enables blind to detect object with ease. It consists of two ultrasonic sensors along with buzzer and vibration motor to notify the user.

**ADVANTAGES**

* Light weight.
* portable.
* Requires very low skill to handle.
* Convenient to use.

***SYSTEM REQUIREMENTS***

**CHAPTER 3**

**SYSTEM REQUIREMENTS**

**3.1 HARDWARE REQUIREMENTS**

* ESP 32 : Micro controller (controls the system).
* Ultrasonic sensor : To detect the nearby object.
* Vibration motor : To notify the user.
* Buzzer : To notify the user.
* Wires : To complete the circuit.
* GPS module : To fetch user current location.

**3.2 SOFTWARE REQUIREMENTS**

* Language Used : C++
* Platform : Arduino IDE

***PROJECT DECRIPTION***

**Chapter 4**

**PROJECT DESCRIPTION**

**4.1 PROJECT DECRIPTION**

The goal of the project is to develop a system which is used by blind to navigate to places easily.The system uses a pair of ultrasonic sensor to detect the object. Once any object is detected, it notifies the user with buzzer sound and vibration pulses. In case of any emergency , the user can expose their current location to the target by pressing a push button. The location is fetched using GPS module.

**4.2 MODULE DESCRIPTION**

The “IoT BASED THIRD EYE FOR VISUALLY CHALLENGED PEOPLE” system will be developed using ESP 32 as microcontroller as the microcontroller and Arduino as programming platform. The application will have three modules, each with a specific function are.

* Object Detection.
* Buzzer and Vibration notification.
* Sending SOS message.

**4.2.1 Object detection**

* In object detection phase the nearby objects are detected by the ultrasonic sensor.
* Once an object is detected the sensors transmits signal to the micro controller.

**4.2.2 buzzer and vibration notification**

* In detection phase the microcontroller makes the buzzer and vibration motor to produce their corresponding output.
* These outputs will notify the user about the incoming objects in his path.

**4.2.3 SENDING SOS MESSAGE**

* In case of emergency, the user can send SOS message to the target what’s app number along with his current location.
* The user current location is fetched using GPS module.
* The location is sent to the target what’s app number using Twilio API.
* Hence the location of the blind can be found with ease.

***SYSTEM DESIGN***

**CHAPTER 5**

**SYSTEM DESIGN**

**5.1 WORKING FLOW DIAGRAM**

ESP32

MICRO-CONTROLLER

ULTRASONIC SENSOR

***SOFTWARE DESCRIPTION***

**CHAPTER 6**

**SOFTWARE DESCRIPTION**

**6.1 SOFTWARE DESCRIPTION**

The various software used in the existing system are :

* Arduino IDE.
* Twilo API.

**6.1.1 ARDUINO IDE**

Arduino IDE is an open-source software, designed by Arduino.cc and mainly used for writing, compiling & uploading code to almost all Arduino modules. It is an official Arduino software, making code compilation too easy that even a common person with no prior technical knowledge can get their feet wet with the learning process.

**6.1.2 TWILIO API**

Twilio API power its platform for communications. Behind these APIs is a software layer connecting and optimizing communications network around the world to allow users to call and message anyone, globally.

It uses REST API(Representational State Transfer) is an architecture pattern that describes how distributed system can expose a consistent interface. In are general ‘REST API’ means an API accessed using the HTTP protocol at a predefined set of URLs.

**6.3 MANAGE CODE**

Arduino IDE provides a user-friendly interface for managing and developing code for Arduino microcontroller boards. The IDE includes several features and tools to help users write, compile, and upload code to the Arduino board.

To manage code in the Arduino IDE, users typically follow the following steps:

* Open the Arduino IDE and create a new sketch. The sketch is the file that contains the code for the Arduino board.
* Write the code for the Arduino board using the built-in text editor. The IDE includes features such as syntax highlighting and autocompletion to make coding easier.
* Verify and compile the code by clicking on the "Verify" button. This checks the code for errors and ensures that it is compatible with the Arduino board.
* Upload the code to the Arduino board by clicking on the "Upload" button. This transfers the code to the board and allows it to be executed.
* Monitor the output of the code by viewing the message console. This displays any debug information or output from the Arduino board.
* Test and refine the code as necessary. The IDE allows users to modify and refine the code as needed, and then repeat the process of verifying, compiling, and uploading the code.

### 6.4 MANAGE DATA

Arduino IDE provides several ways to manage data when programming and developing code for Arduino microcontroller boards. Here are some ways to manage data in the Arduino IDE:

* Variables: Arduino allows users to declare and use variables, which are used to store data such as numbers, text, or Boolean values. Variables can be declared as global or local, depending on their scope.
* Arrays: Arrays are used to store multiple values of the same type.
* Constants: Constants are values that cannot be changed during runtime. They are typically used to store data such as pin numbers or other configuration settings.
* Serial communication: Arduino supports serial communication, which allows users to send and receive data between the microcontroller board and a computer or other device. This is often used for data logging or to interface with external sensors.
* Libraries: Arduino includes a library of pre-written code that can be used to manage data, such as the Wire library for I2C communication or the SD library for reading and writing data to an SD card.

### 6.5 COMMON LANGUAGE SPECIFICATION

The Common Language Specification (CLS) is a set of rules and guidelines for programming languages, including the Arduino programming language. It is designed to ensure that code written in different programming languages can be easily used and interchanged.

### 6.7 ARCHITECTURE OF ARDUINO IDE

The architecture of the Arduino IDE (Integrated Development Environment) can be divided into two main components: the front-end and the back-end.

**6.7.1 FRONT-END:**

The front-end of the Arduino IDE is responsible for providing the user interface and editing capabilities. It is built using the Java programming language and relies on the Swing toolkit for its graphical user interface (GUI). The front-end also manages the compilation and upload process, as well as the communication with the Arduino board.

**6.7.2 BACK-END:**

The back-end of the Arduino IDE is responsible for compiling the user's code into machine-readable instructions that can be uploaded to the Arduino board. It consists of a number of components, including the Arduino core libraries, the AVR toolchain (which includes the compiler, linker, and other tools), and a set of protocols for communicating with the board.

***SYSTEM TESTING***

**CHAPTER 7**

**SYSTEM TESTING**

**7.1 SYSTEM TESTING:**

The purpose of testing is to discover errors in testing and discovering conceivable fault or weakness in a working product if provides a way to check the functionality of components, subassemblies or a finished product. It is the process of exercising software with the intent of ensuring that the Software system meets its requirements and user expectations and does not fail in an unacceptable manner. There are various types of testing Each test type addresses a specific testing requirement.

**7.2 TYPES OF TESTS:**

* Unit Testing .
* Integration Testing .
* Performance Testing.
* Security Testing .

**7.2.1-UNIT TESTING:**

Unit testing is an important part of ensuring that the individual learning system for malware detection correctly and producing the expected outputs. By testing each component in isolation. Developers can identify and address issues early on, before they larger problems in the overall systems.

**7.2.2INTERGRATION TESTING**

Integration testing is an important part of ensuring that the different components of the machine learning systems for malware detection are working together as expected. By testing the integration of different components, developers can identify address issues early on, before they become big problems in the overall system.

**7.2.3PERFOEMANCE TESTING**

* Testing the system's processing speed.
* Testing the system's accuracy .
* Testing the system's scalability .
* Testing the system's resource usage.

**7.2.4 SECURITY TESTING**

Security testing is an important part of ensuring that the machine learning system for malware detection is secure and that it is protecting user data and system resources from different types of attacks. By testing the system's resilience to different types of attacks and its data protection mechanisms. developers can identify and address any security vulnerabilities early on, before they become larger problems in the overall system.

***SYSTEM IMPLEMENTATION***

**CHAPTER 8**

**SYSTEM IMPEMENTATION**

**8.1 SYSTEM IMPEMENTATION**

* Circuit Design and Assembly
* Programming the Microcontroller
* Integration with drivers
* Deployment and Monitoring

**8.1.1 CIRCUIT DESIGN AND ASSEMBLY:**

Design the circuit layout based on the selected components. Connect the microcontroller to the ultrasonic sensor. Ensure proper wiring and connections to avoid any short circuits or malfunctions.

**8.1.2 PROGRAMMING THE MICROCONTROLLER:**

Write the firmware code for the microcontroller. Implement algorithms to read data from the ultrasonic sensor. Program the microcontroller to control the buzzer, vibration motor and GPS module.

**8.1.3 INTEGRATION WITH TWILIO API:**

Once the circuit is designed, integrate the GPS module with the Twilio API. So that the last module “Sending SOS message in case of emergency” can be implemented.

**8.1.4 DEPLOYMENT AND MONITORING:**

Deploy the Drowsiness detection glass with IoT in targeted areas. Monitor system performance and functionality over time. Address any technical issues or maintenance requirements as they arise.

# 

# ***SYSTEM MAINTENANCE***

**CHAPTER 9**

**SYSTEM MAINTENANCE**

**9.1 SYSTEM MAINTENANCE**

**9.1.1 HARDWARE CHECK**

Inspect the I/o devices such as sensors, cameras, or any wearable tech to ensure they are functioning correctly.

**9.1.2 SOFTWARE CHECK**

Check for any software updates for the IoT devices and the central system. Install updates to ensure security and performance enhancements.

**9.1.3 DATA MANAGEMENT**

Review the data collected by the system to ensure it’s accurate and relevant. Clean up any unnecessary data to optimize storage and processing.

**9.1.4 BATTERY MANAGEMENT**

The whole system is powered by using a 3.7v lithium ion battery. It should be charged regularly and completely changed when required.

# ***CONCLUSION & FUTURE ENHANCEMENT***

**CHAPTER 10**

**CONCLUSION & FUTURE ENHANCEMENT**

**10.1 CONCLUSION**

Our project is successfully removing the problem of existing navigation techniques like carry stick with us while walking, use of another person while moving one place to another and many more issue was successfully resolved by this project. The project has the feature to detect the distance of objects that are major issue for blind people after detecting the object distance they also know about the direction where the object was.

**10.2 FUTURE ENHANCEMENT**

The project can be improved as follow in the future :

* 180 degrees coverage.
* Sending SMS to the target phone number.
* Different tone for buzzer and and different vibration intensity for vibration motor for detecting object at different direction.